### 00.00.00 Central extract unit DucoBox Silent UK 3-pin plug

serial no. 1

##### Description:

DucoBox Silent UK 3-pin plug, centrally/non-locally controlled mechanical central extract unit.

##### Operation:

Wireless communication via RF protocol with other control components within the DUCO network.

##### Material:

Plastic: Polypropylene

Electric motor: Supply voltage (VAC): 230

 Absorbed power (W): max. 84.39

 Type: direct current

 Thermally protected

##### Design:

Colour: Green with white cover

Connectors: Diameter (mm): 125

 No. on extraction side: 1

 No. on supply side: 7

##### Technical specifications

Flow (m³/h): Max. 400

Head (Pa): 150

Dimensions (L x W x H) (mm): 480 x 480 x 195

Weight: 4.3 kg

Sound power level (dB(A)) (at 350 m³/h with a head of 100 Pa): Supply: 57.5

 Emission from casing: 46.5

**Accessories:**

With G Plug power cord (3 x 0.75 mm²/2 m) (standard).

Silent Plus Kit (optional with Duco Silent System):

 3 acoustic blocks in central extract unit.

3 acoustic caps on central extract unit.

##### Application:

Mechanical ventilation installation:

Employed as standard in the Duco Silent System.

##### Fitting:

Fitting method: In an enclosed installation location against a wall with a mass > 200 kg/m²

Connectors: Extraction side: fit non-flexible, fixed ducts leading to the outside, the route of which should be as straight and direct as possible; increase in diameter: 125 mm to 160 mm. Use at least 2 extraction openings on the central extract unit, one for ventilating the kitchen and one for ventilating other rooms.

Connection method: Contact your regional dealer or the project department of DUCO Ventilation & Sun Control for commercial and technical assistance (assembly and installation instructions).